|  |  |  |
| --- | --- | --- |
| District I1625 N. French Dr., Hobbs, NM 88240District II811 S. First St., Artesia, NM 88210District III1000 Rio Brazos Road, Aztec, NM 87410District IV1220 S. St. Francis Dr., Santa Fe, NM 87505 | State of New MexicoEnergy, Minerals and Natural Resources DepartmentOil Conservation Division1220 South St. Francis Dr.Santa Fe, NM 87505 | Submit Originalto AppropriateDistrict Office |

**GAS CAPTURE PLAN**

Date:

[ ]  Original Operator & OGRID No.:

[ ]  Amended - Reason for Amendment:

This Gas Capture Plan outlines actions to be taken by the Operator to reduce well/production facility flaring/venting for new completion (new drill, recomplete to new zone, re-frac) activity.

*Note: Form C-129 must be submitted and approved prior to exceeding 60 days allowed by Rule (Subsection A of 19.15.18.12 NMAC).*

**Well(s)/Production Facility – Name of facility**

The well(s) that will be located at the production facility are shown in the table below.

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| Well Name | API | Well Location (ULSTR) | Footages | Expected MCF/D | Flared or Vented | Comments |
|  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |

**Gathering System and Pipeline Notification**

Well(s) will be connected to a production facility after flowback operations are complete, if gas transporter system is in place. The gas produced from production facility is dedicated to Gas Transporter and will be connected to Gas Transporter low/high pressure gathering system located in \_\_\_\_\_\_\_ County, New Mexico. It will require \_\_\_\_\_\_' of pipeline to connect the facility to low/high pressure gathering system. Operator provides (periodically) to Gas Transporter a drilling, completion and estimated first production date for wells that are scheduled to be drilled in the foreseeable future. In addition, Operator and Gas Transporter have periodic conference calls to discuss changes to drilling and completion schedules. Gas from these wells will be processed at Gas Transporter Processing Plant located in Sec.\_\_\_\_\_, Twn.\_\_\_\_\_, Rng.\_\_\_\_\_, \_\_\_\_\_\_\_ County, New Mexico. The actual flow of the gas will be based on compression operating parameters and gathering system pressures.

**Flowback Strategy**

After the fracture treatment/completion operations, well(s) will be produced to temporary production tanks and gas will be flared or vented. During flowback, the fluids and sand content will be monitored. When the produced fluids contain minimal sand, the wells will be turned to production facilities. Gas sales should start as soon as the wells start flowing through the production facilities, unless there are operational issues on Gas Transporter system at that time. Based on current information, it is Operator’s belief the system can take this gas upon completion of the well(s).

Safety requirements during cleanout operations from the use of underbalanced air cleanout systems may necessitate that sand and non-pipeline quality gas be vented and/or flared rather than sold on a temporary basis.

**Alternatives to Reduce Flaring**

Below are alternatives considered from a conceptual standpoint to reduce the amount of gas flared.

* Power Generation – On lease
	+ Only a portion of gas is consumed operating the generator, remainder of gas will be flared
* Compressed Natural Gas – On lease
	+ Gas flared would be minimal, but might be uneconomical to operate when gas volume declines
* NGL Removal – On lease
	+ Plants are expensive, residue gas is still flared, and uneconomical to operate when gas volume declines